SEQUENCE

When Start Button pressed, the platform up & suction on

The sensor on (Platform), then the motor rotates forward.

The 2nd sensor on (Catch) suction pick up the object then motor stop, platform down, arm cylinder goes forward.

Then arm forward sensor on then suction release object, then arm cylinder goes back.

Arm backward sensor on, then the platform up & motor forward then continues the operation.